TekVisa.h

The method for operating Tektronix OSC including:

Basic:

1. Find dev
2. Open dev
3. Send command
4. Read data
5. Query code
6. Write buf
7. Read buf
8. Query buf
9. SRQ
10. Close dev

Advanced:

1. Get ID
2. Get OSC type
3. Connect OSC
4. Disconnect
5. Query waveform header
6. Horizontal setting(including delay, scale, div, recordlength, resolution, trigger pos, zoom function\_
7. Math
8. Measurement
9. Date, Reset, Header off, lock, LRN, SAVe settings
10. Status and error, SRQ etc.
11. Trigger
12. Vertical setting
13. Waveform